**LOT 11: Supply of Personal Protective Equipment (PPE) for beneficiaries of the Rural Youth Employment Support (R-YES) Project (to be used during training).**

*Bidders are expected to examine carefully and comply with all instructions and specifications.*

**Date: \_\_\_\_\_\_/\_\_\_\_\_\_/\_\_\_\_\_\_\_\_\_**

**Bidder Information**

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
| Bidder’s Legal Name |  |  |
|  |
| TIN Number |  |  |
|  |  |  |
| Country/ies of Registration/Operation |  |  |
|

|  |
| --- |
|  |

Bidder’s Authorized Representative |
|  |  |  |  |  |
| Title |  |  Telephone |  |  |
|  |
| Email |  |  |
|  |

**Descriptions and Specifications of required Personal Protective Equipment (PPE) to be supplied to IPRCs.**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S/No** | **Item Description** | **Item Specifications** | **Units** | **Quantity** | **Unit Price (Frw)** | **Total Price (Frw)** |
|  | White R-YES branded overcoat for trainees & trainers | White in colorDifferent seize, small, medium & large  | pc | 260 |  |  |
|  | Grey R-YES branded overcoat for trainees & trainers | Color: GreyTwo pieces work overalls, lightweight.ComposizioneT/C twill, 65% polyester, 35% cotton, 180 g/m2Design• Inserts and knee pads made of “Oxford” polyester/PU, 220 g/m2• Cuffs with strap adjusters• Front strap closure with flap-covered double tap zip• Stretch waistband• Chest pockets with strap closure and pen pocket• Two deep front pockets with small tool inserts with strap closure• Large left-side pocket with strap closure, mobile phone pocket and badge insert• Large rear pockets with "Oxford" reinforcement and strap closure• Ruler pocket and hammer loop• Knee pad inserts | pc | 130 |  |  |
|  | Dark Blue R-YES branded overcoat for trainees & trainers | Color: Dark BlueTwo pieces work overalls, lightweight.ComposizioneT/C twill, 65% polyester, 35% cotton, 180 g/m2Design• Inserts and knee pads made of “Oxford” polyester/PU, 220 g/m2• Cuffs with strap adjusters• Front strap closure with flap-covered double tap zip• Stretch waistband• Chest pockets with strap closure and pen pocket• Two deep front pockets with small tool inserts with strap closure• Large left-side pocket with strap closure, mobile phone pocket and badge insert• Large rear pockets with "Oxford" reinforcement and strap closure• Ruler pocket and hammer loop• Knee pad inserts | Pc | 260 |  |  |
|  | White head covers for trainees & trainers | White in color, cotton | Pc | 130 |  |  |
|  | Industrial helmets for trainees & trainers | SF-06 industrial helmet, ABS material, overhead working, high impact resistance and electrical insulation | Pc | 130 |  |  |
|  | Gloves | Single use, surgical gloves | Cartons  | 20 |  |  |
|  | Rubber Gloves | Latex Reusable Rubber Gloves for Cleaning, Disinfecting, and Dishwashing | Pairs | 195 |  |  |
|  | Assembly gloves | Safety gloves, Comfort Stretch Fit, Power Grip, Smart Touch, Durable Foam Coated | Pairs | 130 |  |  |
|  | Welding safety glasses | Welding safety glasses - SG-25WS5 – ELVEX Corporation -polycarbonate | Pcs | 130 |  |  |
|  | White Gumboots | white in color, plastic, chemical resistant, number of wearing:6,7,8,9,10, internal side made by fiber, not slippery on the floor, do not Wet feet, do not impact, and crushes in the toe area | Pairs | 260 |  |  |
|  | Protective shoes | Width steel toe cap safety gumboots, PVC Material. Black, 330 mm heightDifferent size: Wearing number 7,8,9,10,11,12 | Pairs | 195 |  |  |
|  | Protective shoes | American safety boot with different seize from 8 to 11 | Pairs | 6 |  |  |
|  | Protective shoes (for industrial use) | High cut light weight industrial safety shoes, acid and alkali resistant waterproof. Leather upper shoe materialDifferent size: Wearing number 7,8,9,10 | Pairs | 195 |  |  |
|  | White Socks | White, long  | Pairs  | 130 |  |  |
|  | Grey, Dark blue or Black socks | Grey, Dark blue or Black, long  | Pairs  | 520 |  |  |

**NOTE:**

Kilimo Trust Rwanda, in a fair and transparent manner, will select companies that fulfill all requirements.